**CG2271 lab 7 Report**

**Q1.** What is the default priority level at which the led\_green\_thread is created?

The default priority for green led is osPriorityNormal

**Q2.** What are the highest and lowest priority levels that can be assigned to a task?

The lowest priority is osPriorityNone and the highes priority is osPriorityReserved

**Q3**. State your observation. Explain why you see such a behaviour.

We observed that only the red led will light up as the priority is set as osPriorityNormal1 which is higher than the green led which is osPriorityNormal.

**Q4.** Describe your observation. Explain why it is as such.

**Q5.** Describe your observation. Explain why it is as such.